Please refer to PART 1: VORTEX GENERAL CLAUSES for all Play Product construction and installation information.

1. Play Product Specifications:
	1. Play Product Structure:The Gusher VOR-300.4000 shall be constructed of 304/304L stainless steel with an outside diameter of 4½" (11.4cm). The brass spray cap shall be fastened to the gusher body using tamper-resistant fasteners. Tamper resistant brass winter cap shall be included. The anchoring system shall have an integrated levelling system facillitating installation and a plumb finished to the activity deck surface. Ground Sprays can be fitted with several interchangeable compatible spray head styles however, The spray zone layouts between the different products must be similar or must be planned to accommodate the various spray effects. When multiple ground sprays are plumbed together on a single water line, the connected ground sprays must have similar hydraulic requirements.

* 1. Overall play product dimensions**:** The overall height of the Play Product shall be 0" (0 cm) above ground.
	2. Play Product Interactivity: Users can feel the more powerful water spray near the ground, and lighter pressure near the top of the gusher.
	3. Hydraulic Activity/Components: The spray cap shall have a thirty-six (36)-hole spray pattern angled at 5° from vertical so that multiple streams spray water straight up from a concentrated circle.
	4. Hydraulic Requirements:The hydraulic requirements shall be 11-17 gpm (42-64 lpm) @ 3-6 psi (0.1 – 0.3 bar).