Please refer to PART 1: VORTEX GENERAL CLAUSES for all Play Product construction and installation information.

1. Play Product Specifications:
   1. Play Product Structure:The Geyser N°2 VOR-331.4000 shall be constructed of 304/304L with an outside diameter of 3" (7.62cm). The brass spray cap shall be threaded into the geyser body using a tamper-resistant tool. Tamper resistant brass winter cap shall be included. The anchoring system shall have an integrated levelling system facillitating installation and a plumb finished to the activity deck surface.

* 1. Overall play product dimensions**:** The overall height of the Play Product shall be 0" (0 cm) above ground.
  2. Play Product Interactivity: Users can touch the soft frothy water falling down in contrast to the more powerful streams spraying up from the centre.
  3. Hydraulic Activity/Components: The spray cap shall have a ten (10)-hole spray pattern angled at 5° (degrees) from vertical so that multiple streams spray water out at symmetrical angles forming an elegant geyser effect.
  4. Hydraulic Requirements:The hydraulic requirements shall be 5-15 gpm (19-57 lpm) @ 3-8 psi (0.2-0.6 bar).