Please refer to PART 1: VORTEX GENERAL CLAUSES for all Play Product construction and installation information.

1. Play Product Specifications:
	1. Play Product Structure:The Cascade Loop VOR-7250 shall include two (2) Basins, three (3) Play Ponds, two (2) molded polymer ORBS and four (4) Waves. The Basins assembly: shall be constructed of curved tubing made of 304/304L stainless-steel structural tubing with an outside diameter of 2.375” (60mm) and a wall thickness of 0.109” (2.8mm). The overall height of Basins assembly shall be no less than 32.5” (82.5cm). The Play Pond structures shall be constructed of curved tubing made of 304/304L stainless-steel with an outside diameter of 3.50” (8.9cm) and a wall thickness of 0.12” (3.0mm) and stainless-steel sheet pieces of thickness ¼” (6.3mm). The Basins shall be constructed of 3/16” (4.7mm) translucent SEEFLOW™ polymer. The Play Ponds and Waves shall be constructed of 1/2” (12.7 mm) translucent SEEFLOW™ polymer. The two ORBS and four Waves spin freely by means of a mechanism of low friction polymer bushings and are propelled to spin by the force of the water flow or users. The overall height of the top Play Pond shall be no less than 40.75” (103.5cm). The overall height of the middle Play Ponds shall be no less than 29” (73.6cm). The overall height of the bottom Play Ponds shall be no less than 23” (58.4cm). The Top Play Pond with Basins shall be anchored with a SAFESWAP™ Anchoring System. All other Play Ponds shall be fastened to the surface with mechanical anchors.
	2. Overall play product dimensions**:** The overall height of the Cascade Loop shall be no less than 70.5” (179cm) with a width of 73.5” (186.7cm) and a length of 71.5” (181.6cm).
	3. Play Product Interactivity: Users must work together to keep the water flowing from one Play Pond to the next to keep the ORBS spinning. Giving everyone a chance to participate and encouraging team play. Users can also interact with the ORBS and Waves to splash around.
	4. Hydraulic Activity/Components: The Cascade Loop top Basin shall be filled with water from the water line connection and then cascade into the next Basin without overflow. The bottom Basin will cascade down the water into the top Play Pond. Water will flow in both direction of the top Pond to activate the Orb from the Play Ponds below and cascade down until it reaches the floor.
	5. Hydraulic Requirements:The hydraulic requirements shall be 4-6 gpm (15-23 lpm) @ 3-4 psi (0.2-0.3 bar).