Please refer to PART 1: VORTEX GENERAL CLAUSES for all Play Product construction and installation information.

1. Play Product Specifications:
   1. Play Product Structure:The Tall Grass N°1, shall consist of a curved base support post made of 304/304L stainless steel tubing with an outside diameter of 3.50” (8.9cm) and a wall thickness of 0.30” (7.6mm). All bending shall have no joint or ripples. The two sides will each have a SEEFLOW™ polymer panel attached using tamper-resistant fasteners. A total of four (4) soft mist spray effect. The nozzles shall be free of finger entrapment hazards. The SAFESWAP™ anchoring and leveling system shall be used. The TOEGUARD™ will then be added to protect children's toes from anchoring hardware.
   2. Overall play product dimensions**:** The overall height of the Play Product shall be 75" (190 cm) above ground.
   3. Play Product Interactivity: Tall Grass N°1 shall create visual interest as water mists from multiple places along the curvy post.
   4. Hydraulic Activity/Components: Each nozzle shall produce a spray mist effect.
   5. Hydraulic Requirements:The hydraulic requirements shall be 5-10 gpm (18.90-37.80 lpm) @ 8-12 psi (0.55-0.83 bar).