Please refer to PART 1: VORTEX GENERAL CLAUSES for all Play Product construction and installation information.

1. Play Product Specifications:
	1. Play Product Structure:The Ombrello No1 VOR-7445.2009 shall consist of one (1) Post and one (1) SEEFLOW™ Ombrello Dome. The Post shall be upright and constructed of stainless steel structural tubing with an outside diameter of 3.50" (8.9cm) and a wall thickness of 0.12" (3.0mm). The SEEFLOW™ Ombrello Dome shall have a diameter of 36" (91cm) and shall be constructed of translucent SEEFLOW™ polymer with a center stainless steel spray cap.The SAFESWAP™ anchoring and leveling system shall be used.

* 1. Overall play product dimensions**:** The overall height of the Ombrello No1 shall be no less than 122” (310cm) above final grade.
	2. Play Product Interactivity: Creates visual interest as water sprays from the top and streams down over the translucent SEEFLOW™ Ombrello Dome.
	3. Hydraulic Activity/Components: Eight (8) gentle water streams emitted from the center spray cap shall flow down over the SEEFLOW™ Ombrello Dome.
	4. Hydraulic Requirements:The combined hydraulic requirements shall be 5-6 gpm (19-27 lpm) @ 5-6 psi (0.34-0.41 bar).