Please refer to PART 1: VORTEX GENERAL CLAUSES for all Play Product construction and installation information.

1. Play Product Specifications:
   1. Play Product Structure:The Jet Stream N°1 VOR-7512.0000 shall be constructed of 304/304L stainless steel structural tubing with an outside diameter of 3" (7.6cm). The lead-free brass spray cap shall be threaded into the stainless steel spray head housing using a tamper-resistant tool. Tamper resistant brass winter cap shall be included. The Embedded anchoring and leveling system shall be used.

* 1. Overall play product dimensions**:** The overall height of the Play Product shall be 0" (0 cm) above ground.
  2. Play Product Interactivity: Creates visual interest as a concentrated jet of water sprays up in a sleek Jet Stream.
  3. Hydraulic Activity/Components: The lead-free brass spray cap shall have a single ¼” (6mm) spray hole projecting a vertical stream.
  4. Hydraulic Requirements:The hydraulic requirements shall be 2-3 gpm (7.6 – 11.3 lpm) @ 5-10 psi (0.4 – 0.7 bar).