Please refer to PART 1: VORTEX GENERAL CLAUSES for all Play Product construction and installation information.

1. Play Product Specifications:
   1. Play Product Structure:The Fountain Spray Nº1 VOR-7513.0000 shall be constructed of 304/304L stainless steel structural tubing with an outside diameter of 3" (7.6cm). The lead-free brass spray cap shall be threaded into the stainless steel spray head housing using a tamper-resistant tool. Tamper resistant brass winter cap shall be included. The Embedded anchoring and leveling system shall be used.

* 1. Overall play product dimensions**:** The overall height of the Play Product shall be 0" (0 cm) above ground.
  2. Play Product Interactivity: Users can experience a variety of water effects: the gentle streams falling down, mist from under the water arcs and higher pressure at the core.
  3. Hydraulic Activity/Components: The lead-free brass spray cap shall have an eleven (11)-hole spray pattern, three (3) holes angled at 5° from vertical and eight (8) holes angled at 10° from vertical.
  4. Hydraulic Requirements:The hydraulic requirements shall be 3-7 gpm (11.4 – 26.5 lpm) @ 1-4 psi (0.07 – 0.28 bar).