Please refer to PART 1: VORTEX GENERAL CLAUSES for all Play Product construction and installation information.

1. Play Product Specifications:
	1. Play Product Structure:The Cattail VOR-7538.2008 shall be constructed of bent 304/304L stainless steel structural tubing with an outside diameter of 3½" (8.9cm) and a wall thickness of 0.120" (3mm). The top extremity of the tail consist of one (1) translucent SEEFLOW™ polymer flower head. Four (4) nozzles are inserted around along the body post. All nozzle are to be flush with the surface to eliminate finger entrapment and protrusion hazards. The SAFESWAP™ anchoring and leveling system shall be used.

* 1. Overall play product dimensions**:** The overall height of the play structure shall be 129" (328cm) above ground.
	2. Play Product Interactivity: Users can enjoy the four (4) streams that spray from the Cattail.
	3. Hydraulic Activity/Components: The four (4) nozzles on the post of the Cattail shall produce a soft stream spray effect.
	4. Hydraulic Requirements:The combined Hydraulic requirements shall be 2-4 gpm (8-15 lpm) @ 5-6 psi (0.3-0.4 bar).