Please refer to PART 1: VORTEX GENERAL CLAUSES for all Play Product construction and installation information.

1. Play Product Specifications:
	1. Play Product Structure:The Flower No. 1 VOR-7549.2009 shall be constructed of 304/304L stainless steel structural tubing with an outside diameter of 4½" (11.4cm) and a wall thickness of .120" (3mm). The post shall be curved with no joints or ripples. At the top extremity a 30” (76cm) diameter water dome shall be attached. It is made of translucent SEEFLOW™ polymer. The SAFESWAP™ anchoring and leveling system shall be used.

* 1. Overall play product dimensions**:** The overall height shall be 135” (342cm) above final grade and shall span 28” (70cm) in width with a head clearance of 96" (244cm).
	2. Play Product Interactivity: Users can enjoy the reflection of sunlight and water on the translucent water dome of the flower.
	3. Hydraulic Activity/Components: The flower No. 1 produce a continous flow.
	4. Hydraulic Requirements:The combined hydraulic requirements shall be 5-25 gpm (19-95 lpm) @ 5-10 psi (0.3-0.7 bar).