Please refer to PART 1: VORTEX GENERAL CLAUSES for all Play Product construction and installation information.

1. Play Product Specifications:
	1. Play Product Structure:The Flower No.2 VOR-7550.2008 shall be constructed of 304/304L stainless steel structural tubing with an outside diameter of 4½" (11.4cm) and a wall thickness of .120" (3mm), with a side arm constructed of 3½” (89mm) outside diameter 304/304L stainless steel structural tubing with wall thickness of .120” (3mm). The side arm shall be welded on the main post. The main post and the side arm shall be curved with no joints or ripples.The water flower shall have a diameter of 30” (76cm) and shall be constructed of translucent SEEFLOW™ polymer with an Ultra High Molecular Weight Polyethylene center spray cap. The water dome shall be 30” (76cm) in diameter and be made of translucent SEEFLOW™ polymer. The SAFESWAP™ anchoring and leveling system shall be used.

* 1. Overall play product dimensions**:** The overall height shall be 135” (342cm) above final grade and shall span 30” (76cm) in width with a head clearance of 96" (244cm).
	2. Play Product Interactivity: Users can enjoy the reflection of sunlight and water on the translucent water dome and water flower.
	3. Hydraulic Activity/Components: The flower No. 2 produce a continous flow.
	4. Hydraulic Requirements:The combined hydraulic requirements shall be 15-30 gpm (56-114 lpm) @ 5-10 psi (0.3-0.7 bar).