Please refer to PART 1: VORTEX GENERAL CLAUSES for all Play Product construction and installation information.

1. Play Product Specifications:
	1. Play Product Structure:The Fountain Spray N°2 VOR-7676.4000 shall be constructed of 304/304L stainless steel structural tubing with an outside diameter of 3" (7.6cm). The lead-free brass spray cap shall be threaded into the stainless steel spray head housing using a tamper-resistant tool. Tamper resistant brass winter cap shall be included. The Embedded anchoring and leveling system shall be used.

* 1. Overall play product dimensions**:** The above ground height of the Play Product shall be 0" (0 cm).
	2. Play Product Interactivity: Creates excitement as a blast of water erupts from the Fountain Spray N°2, shooting up a stream of water. Users can move a hand or leg through the water to feel the power.
	3. Hydraulic Activity/Components: A lead-free brass spray head nozzle shall be mounted flush with the surface of the volcano nose cap and shall produce six (6) particularized, soft stream spray effects.
	4. Hydraulic Requirements:The hydraulic requirements shall be 1-5 gpm (4 – 19 lpm) @ 5-10 psi (0.4 – 0.7 bar).