Please refer to PART 1: VORTEX GENERAL CLAUSES for all Play Product construction and installation information.

1. Play Product Specifications:
   1. Play Product Structure:The Silhouette No1 VOR-7772.2008 shall be constructed of 304/304L stainless steel structural tubing with an outside diameter of 4½" (11.4cm) and a wall thickness of .120" (3mm). It shall have a curvy bend with no ripples or joints. The SAFESWAP™ anchoring and leveling system shall be used.

* 1. Overall play product dimensions**:** The above ground height of the structure shall be no less than 40" (102cm) height.
  2. Play Product Interactivity: Users can watch the bell shaped spray and touch the laminar texture of the water.
  3. Hydraulic Activity/Components: The spray effect shall be a clear, laminar bell shaped, sheet descending from the top of the post towards grade.
  4. Hydraulic Requirements:The hydraulic requirements shall be 25-40 gpm (95-151 lpm) @ 2-4 psi (0.1 – 0.3 bar).